QA - Andrzej and Robert

|  |
| --- |
| STAGE ONE - HARDWARE  RASPBERRY PI  CAMERA  MOTION DETECTOR |
| STAGE TWO - ACCESS / RUN VIA COMMAND LINE INTERFACE (CLI)  LOAD TERMINAL and SSH into RASPBERRY |
| STAGE - AWS PORTAL NO IMAGES  STAGE - AWS PORTAL UPLOADED IMAGES |
| STAGE - MOTION DETECTION |